**Drawing Name Description**

KCDD011 Sheet 01 of 12 Typical Details with Perimeter Pressure Plate

KCDD011 Sheet 02 of 12 Typical Details with "F-Perimeter"

KCDD011 Sheet 03 of 12 Typical Details with Perimeter Mullions

KCDD011 Sheet 04 of 12 Typical 90° & 135° Corner / Splayed Mullion Details

KCDD011 Sheet 05 of 12 Windows and GLASSvent® Windows for Curtain Wall Details

KCDD011 Sheet 06 of 12 Entrance Details - Center Hung with Concealed Overhead Closer

KCDD011 Sheet 07 of 12 Entrance Details - Offset Pivot/Butt Hung with Single Acting COC or Surface Closer

KCDD011 Sheet 08 of 12 Entrance Details - Offset Pivot/Butt Hung with LCN 2030/5030 COC or Surface Closer

KCDD011 Sheet 09 of 12 Entrance Details – Heavy Wall™ Offset Pivot/Butt Hung with Single Acting COC or Surface Closer

KCDD011 Sheet 10 of 12 Entrance Details – Heavy Wall™ Offset Pivot/Butt Hung with LCN 2030/5030 COC or Surface Closer

KCDD011 Sheet 11 of 12 Typical Anchor Details & Steel Reinforcing Details

KCDD011 Sheet 12 of 12 Typical Splice Details