**Drawing Name Description**

KCDD080C Sheet 01 of 11 Typical Details with Perimeter Pressure Plate

KCDD080C Sheet 02 of 11 Typical Details with Thermal Pocket Filler

KCDD080C Sheet 03 of 11 90° Corner Details

KCDD080C Sheet 04 of 11 AA™ 6400 Windows and GLASSvent™ UT Window Details

KCDD080C Sheet 05 of 11 Entrance Details - Center Hung with Concealed Overhead Closer

KCDD080C Sheet 06 of 11 Entrance Details - Offset Pivot/Butt Hung with Single Acting Offset Arm COC or Surface / Floor Closer

KCDD080C Sheet 07 of 11 Entrance Details - Offset Pivot/Butt Hung with Surface or Floor Closer

KCDD080C Sheet 08 of 11 Entrance Details - Offset Pivot/Butt Hung with Single Acting Offset Arm COC, Surface or Floor Closer with 250T Insulpour Thermal Door

KCDD080C Sheet 09 of 11 Entrance Details - Offset Pivot/Butt Hung with Surface or Floor Closer with 250T Insulpour Thermal Door

KCDD080C Sheet 10 of 11 Typical Anchoring Details & Steel Reinforcing Details

KCDD080C Sheet 11 of 11 Typical Splice Details